**REFERENCES ON the Properties of**

**WATER, BRINE AND CO2**

Adams, J. J.; Bachu, S. Equations of state for basin geofluids: algorithm review and intercomparison for brines. *Geofluids* **2002**, *2 (4)*: 257-271.

Altunin, V.V. *Thermophysical Properties of Carbon Dioxide.* Moscow, Russia: Publishing House of Standards, 1975, 551 p. (in Russian)

Barta, L.; Bradley, D. J. Extension of the specific interaction model to include gas solubilities in high temperature brines. *Geochimica et Cosmochimica Acta* **1985**, *49 (1*): 195-203.

Batzle, M.; Wang, Z. Seismic properties of pore fluids. *Geophysics* **1992**, *57 (11)*: 1396-1408.

Burke, L. *Carbon Dioxide Fluid-Flow Modeling and Injectivity Calculations*. Scientific Investigation Report 2011–5083. Reston, VA: U.S. Geological Survey, 2011.

Carroll, J. J.; Slupsky, J. D.; Mather, A. E. The solubility of carbon dioxide in water at low pressure. *Journal of Physical and Chemical Reference Data* **1991**, *20 (6)*: 1201-1209. Accessed on 01 August 2012 @ URL: <http://www.nist.gov/data/PDFfiles/jpcrd427.pdf>

Diamond, L. W; Akinfiev, N. N. Solubility of CO2 in water from -1.5 to 100 oC and from 0.1 to 100 MPa: Evaluation of literature data and thermodynamic modelling. *Fluid Phase Equilibria* **2003**, *208 (1-2)*: 265-290.

Dittman, G. L. *Calculation of brine properties*. Report UCID-17406. Livermore, Calif., U.S. Department of Energy, Lawrence Livermore Laboratory, 1977. Accessed on 01 August 2012 @ URL: <http://www.osti.gov/bridge/servlets/purl/7111583-l9lvkU/native/7111583.pdf>

Doughty, C. West coast regional carbon sequestration partnership, pre-injection modeling in a saline formation in the southern San Joaquin Valley, California. In: NETL (National Energy Technology Laboratory). *Regional carbon sequestration partnerships’ simulation and risk assessment case histories, addendum to best practices for risk analyses and simulation for geologic storage of CO2*. Report DOE/NETL-2011/1459. Pittsburgh, PA: U.S. Department of Energy, National Energy Technology Laboratory, 2011; pp 78-103. Accessed on 26 July 2012 @ URL: <http://www.netl.doe.gov/technologies/carbon_seq/refshelf/BPM_Sim_Risk_Appdx_IV_web.pdf>

Duan, Z.; Sun, R. An improved model calculating CO2 solubility in pure water and aqueous NaCl solutions from 273 to 533 K and from 0 to 2000 bar, *Chemical Geology* **2003**, *193 (3-4)*: 257-271. Accessed on 26 July 2012 @ URL:   
<http://www.geochem-model.org/Publications/28-CG2003-193.pdf>

Duan, Z.; Sun, R.; Zhu, C.; Chou, IM. An improved model for the calculation of CO2 solubility in aqueous solutions containing Na+, K+, Ca2+, Mg2+, Cl-, and SO42-. *Marine Chemistry* **2006**, *98 (2)*: 131–139. Accessed on 26 July 2012 @ URL:   
<http://www.geochem-model.org/Publications/41-MC_98_131.pdf>

Duschek, W.; Kleinrahm, R.; Wagner, W. Measurement and correlation of the (pressure, density, temperature) relation of carbon dioxide I. The homogeneous gas and liquid regions in the temperature range from 217 K to 340 K at pressures up to 9 MPa. *The Journal of Chemical Thermodynamics* **1990**, *22 (9)*: 827-840.

Duschek, W.; Kleinrahm, R.; Wagner, W. Measurement and correlation of the (pressure, density, temperature) relation of carbon dioxide II. Saturated-liquid and saturated-vapour densities and the vapour pressure along the entire coexistence curve. *The Journal of Chemical Thermodynamics* **1990**, 22 (9): 841-864.

E.ON UK 2011. *Equation of state prediction of carbon dioxide properties*. Report KCP-GNS-FAS-DRP-0001, Rev.: 02. Kingsnorth Carbon Capture and Storage Project, Chapter 6.23. Prepared by E.ON UK PLC for United Kingdom’s Department of Energy and Climate Change. Coventry, England: E.ON PLC. Accessed 19 July 2012, at URL: <http://www.decc.gov.uk/assets/decc/11/ccs/chapter6/6.23-equation-of-state-prediction-of-carbon-dioxide-properties.pdf>

Ershaghi, I.; Abdassah, D.; Bonakdar, M. R.; Ahmad, S. Estimation of geothermal brine viscosity. *Journal of Petroleum Technology* **1983**, *35 (3)*: 621-628.

Enick, R. M.; Klara, S. M. CO2 solubility in water and brine under reservoir conditions. *Chemical Engineering Communications* **1990**, *90 (1)*: 23-33.

Fenghour, A.; Wakeham, W. A.; Vesovic, V. The viscosity of carbon dioxide. *Journal of Physical and Chemical Reference Data* **1998**, *27 (1)*: 31-44.

Francke, H.; Thorade, M. Density and viscosity of brine: An overview from a process engineers perspective. *Chemie der Erde - Geochemistry* **2010**, *70* *(Suppl. 3)*: 23-32.

Garcia, J. E. Density of aqueous solutions of CO2. Berkeley, CA: Lawrence Berkeley National Laboratory, 2001. Accessed 13 September 2012, at URL: http://escholarship.org/uc/item/6dn022hb#page-1 .

Han, W. S. *Evaluation of CO2 trapping mechanisms at the SACROC northern platform: site of 35 years of CO2 injection*. PhD Thesis, The New Mexico Institute of Mining and Technology, Socorro, New Mexico, 2008. Accessed 15 August 2012, at URL: <http://www.ees.nmt.edu/outside/alumni/papers/2008d_han_ws.pdf>

Hangx, S. J. T. *Subsurface mineralisation: Rate of CO2 mineralisation and geomechanical effects on host and seal formations. Behaviour of the CO2-H2O system and preliminary mineralisation model and experiments.* CATO – CO2 capture, transport and storage, Report WP 4.1-3-05. Utrecht, Netherlands: Utrecht University, 2005. Accessed on 26 July 2012 @ URL: <http://science.uwaterloo.ca/~mauriced/earth691-duss/CO2_General%20CO2%20Sequestration%20materilas/CO2_Behaviour_of_the_CO2-H2O_system.pdf>

Hassanzadeh, H.; Pooladi-Darvish, M.; Elsharkawy, A. M.; Keith, D. W.; Leonenko, Y. Predicting PVT data for CO2–brine mixtures for black-oil simulation of CO2 geological storage. *International Journal of Greenhouse Gas Control*, **2008**, *2 (1)*: 65-77. Accessed on 27 July 2012 @ URL: <http://www.iapws.org/relguide/IAPWS95-Rev.pdf> <http://www.fekete.com/resources/papers/predicting_pvt_data_co2_paper.pdf>

Haynes, W. M. *CRC handbook of chemistry and physics, 93rd edition*. Boca Raton, FL: CRC Press.

Huber, M. L.; Perkins, R. A.; Laesecke, A.; Friend, D. G.; Sengers, J. V.; Assael, M. J.; Metaxa, I. N.; Vogel, E.; Mareš, R.; Miyagawa, K. New international formulation for the viscosity of H2O. *Journal of Physical and Chemical Reference Data* **2009**, *38 (2)*: 101-125.

IAPWS (International Association for the Properties of Water and Steam). R*evised Release on the IAPWS Formulation 1995 for the Thermodynamic Properties of Ordinary Water Substance for General and Scientific Use*. Doorwerth, Netherlands: International Association for the Properties of Water and Steam, 2009 (Revised 2010). Accessed on 27 July 2012 @ URL: <http://www.iapws.org/relguide/IAPWS95-Rev.pdf>

IAPWS. *Release on the IAPWS Formulation 2008 for the Thermodynamic Properties of Seawater*. Berlin, Germany: International Association for the Properties of Water and Steam, 2008. Accessed on 27 July 2012 @ URL: <http://www.iapws.org/relguide/seawater.pdf>

IOC (Intergovernmental Oceanographic Commission), SCOR (Scientific Committee on Oceanic Research), and IAPSO (International Association for the Physical Sciences of the Oceans). *The international thermodynamic equations of seawater – 2010: calculation and use of thermodynamic properties*. Intergovernmental Oceanographic Commission, Manuals and Guides No. 56. Paris, France: UNESCO (United Nations Educational, Scientific and Cultural Organization), 2010; 196 pp.

ITTC (International Towing Tank Conference) 26th Specialist Committee on Uncertainty Analysis. *Recommended procedures, fresh water and seawater properties*. Procedure 7.5-02-01-03, Revision 2. International Towing Tank Conference. Rio de Janeiro, Brazil, 28 August to 3 September 2011. Accessed 23 July 2012 @ URL: <http://ittc.sname.org/CD%202011/pdf%20Procedures%202011/7.5-02-01-03.pdf>

Jones, G.; Dole, M. The viscosity of aqueous solutions of strong electrolytes with special reference to barium chloride. *Journal of American Chemical Society* **1929**, *51 (10)*: 2950-2964.

Kell, G. S. Density, thermal expansivity, and compressibility of liquid water from 0o to 150o C: Correlations and tables for atmospheric pressure and saturation reviewed and expressed on 1968 temperature scale. *Journal of Chemical and Engineering Data* **1975**, *20 (1)*: 97-105.

Kestin, J.; Sengers, J. V. New international formulations for the thermodynamic properties of light and heavy water. *Journal of Physical and Chemical Reference Data* **1986**, *15 (1)*: 305 – 320.

Kestin, J.; Sengers, J. V.; Kamgar-Parsi, B.; Levelt-Sengers, J. M. H. Thermophysical Properties of Fluid H2O. *Journal of Physical and Chemical Reference Data* **1984**, *13 (1)*: 175-183.

Kestin, J.; Khalifa, H. E.; Correia RJ. Tables of the dynamic and kinematic viscosity of aqueous NaCl solutions in the temperature range 20-150° C and the pressure range 0.1-35 MPa. *Journal of Physical and Chemical Reference Data* **1981**, *10 (1)*: 71-87.

Kestin, J.; Shankland I. R. Viscosity of aqueous NaCl solutions in the temperature range 25−200 °C and in the pressure range 0−130 MPa. International Journal of Thermophysics **1984**, *5 (3)*: 241-263.

Kohl, A.; Nielsen, R. *Gas purification.* Houston TX: Gulf Publishing Company; 1997.

Kumar, A. *A simulation study of carbon sequestration in deep saline aquifers*. MS Thesis, University of Texas at Austin, Austin, Texas, 2004. Accessed 26 July 2012, @ URL: <http://www.pge.utexas.edu/theses04/ajkumar.pdf>

Kwak, H. T.; Zhang, G.; Chen, S. The effects of salt type and salinity on formation water viscosity and NMR responses. (*Paper prepared for Proceedings of the International Symposium of the Society of Core Analysts held in Toronto, Canada, 21-25 August 2005.* Dublin, CA: Society of Core Analysts, 2005.) Accessed 07 July 2012, at URL: <http://www.scaweb.org/assets/papers/2005_papers/1-SCA2005-51.pdf>

Lemmon, E. W.; Huber, M. L.; McLinden, M. O. NIST Standard Reference Database 23: *Reference Fluid Thermodynamic and Transport Properties-REFPROP*, Version 8.0, National Institute of Standards and Technology, Standard Reference Data Program, Gaithersburg, 2007.

Lemmon, E. W.; Huber, M. L..; McLinden, M. O. *NIST Standard Reference Database 23: reference fluid thermodynamic and transport properties-REFPROP, Version 9.0*. Gaithersburg, MD: U.S. Department of Commerce, National Institute of Standards and Technology, Standard Reference Data Program, 2010.

Lewis, K. C.; Lowell, R. P. Numerical modeling of two-phase flow in the NaCl-H2O system: Introduction of a numerical method and benchmarking. *Journal of Geophysical Research* **2009**, *114 (5)*: B05202, 18 p.

Mao, S.; Duan, Z. The P, V, T, x properties of binary aqueous chloride solutions up to T=573K and 100MPa. *Journal of Chemical Thermodynamics* **2008**, *40 (7)*: 1046-1063.

Mao, S.; Duan, Z. The viscosity of aqueous alkali-chloride solutions up to 623 K, 1,000 bar, and high ionic strength. *International Journal of Thermophysics* **2009**, *30 (5)*: 1510-1523.

Michels, A.; Botzen, A.; Schuurman, W. The viscosity of carbon dioxide between 0°C and 75°C and at pressures up to 2000 atmospheres. 155th publication of the Van der Waals Fund Van der Waals-laboratorium, Gemeente Universiteit, Amsterdam, Nederland. *Physica* **2004**, *23 (1–5)*: 1957: 95–102.

McCain, W. D. *The properties of petroleum fluids*. Tulsa, OK: PennWell Books, 1990.

NETL (National Energy Technology Laboratory). *Regional carbon sequestration partnerships’ simulation and risk assessment case histories, addendum to best practices for risk analyses and simulation for geologic storage of CO2.* Report DOE/NETL-2011/1459. Pittsburgh, PA: U.S. Department of Energy, National Energy Technology Laboratory, 2011. Accessed on 26 July 2012 @ URL: <http://www.netl.doe.gov/technologies/carbon_seq/refshelf/BPM_Sim_Risk_Appdx_IV_web.pdf>

Ouyang, L-B. New Correlations for predicting the density and viscosity of supercritical carbon dioxide under conditions expected in carbon capture and sequestration operations. *The Open Petroleum Engineering Journal* **2011**, *4 (1)*: 13-21. Accessed 23 July 2012 @ URL: <http://benthamscience.com/open/topej/articles/V004/13TOPEJ.pdf>

Ozbek, H.; Phillips, SL. *Thermal conductivity of aqueous NaCl solutions from 20oC to 330oC*. Report LBL-9086. Berkeley, CA: U.S. Department of Energy, Lawrence Berkeley Laboratory, Office of Basic Energy Science, Division of Engineering, Mathematical and Geosciences, 1979. Accessed on 01 August 2012 @ URL: <http://www.osti.gov/bridge/servlets/purl/6269880-iPJPhB/6269880.pdf>

Palliser, C.; McKibbin, R. A Model for Deep Geothermal Brines, II: Thermodynamic Properties – Density. *Transport in Porous Media* **1998**, *33 (1-2)*: 129-154.

Palliser, C.; McKibbin, R. A model for deep geothermal brines, III: Thermodynamic properties – enthalpy and viscosity. *Transport in Porous Media* **1998,** *33 (1-2)*: 155-171.

Phillips, S. L.; Igbene, A.; Fair, J. A.; Ozbek, H.; Tavana M. *A technical databook for geothermal energy utilization.* Report LBL-12810. Berkeley, CA: U.S. Department of Energy, Lawrence Berkeley Laboratory, 1981. Accessed on 26 July 2012 @ URL: <http://escholarship.org/uc/item/5wg167jq>

Phillips, S. L.; Otto, R. J.; Ozbek, H.; Tavana, M. Aqueous solutions database to high temperatures and pressures NaCl solutions. Report LBL-9621. Workshop on Techniques for Measurement of Thermodynamic Properties, Albany, OR, 21-23 August 1979. Berkeley, CA: U.S. Department of Energy, Lawrence Berkeley Laboratory, 1979. Accessed on 30 August 2012 @ URL: <http://www.osti.gov/geothermal/servlets/purl/5848013-6op8Lz/native/5848013.pdf>

Phillips, S. L.; Ozbek, H.; Igbene, A.; Litton, G. Viscosity of NaCl and other solutions up to 350o c and 50 MPa pressures. Report LBL-11586. Berkeley, CA: U.S. Department of Energy, Lawrence Berkeley Laboratory, 1980. Accessed on 4 September 2012 @ URL: <http://www.osti.gov/bridge/purl.cover.jsp?purl=/6731414-Tu9XFl/6731414.pdf>

Pistone, S.; Stacey, R.; Horne, R. The significance of CO2 solubility in geothermal reservoirs**.** Proceedings, *Thirty-Sixth Workshop on Geothermal Reservoir Engineering*, Stanford University, Stanford, California, January 31 - February 2, 2011. *Stanford Geothermal Program, Report SGP-TR-191*, 2011. Accessed on 26 July 2012 @ URL: <http://www.geothermal-energy.org/pdf/IGAstandard/SGW/2011/stacey.pdf>

Potter, R. W. II. Viscosity of geothermal brines. *Geothermal Resources Council Transactions* **1978**, *2 (2)*: 543-544.

Portier, S.; Rochelle, C. Modelling CO2 solubility in pure water and NaCl-type waters from 0 to 300oC and from 1 to 300 bar - application to the Utsira Formation at Sleipner. *Chemical Geology*, **2005**, *217 (3–4)*: 187–199.

Pruess, K.; Spycher, N. ECO2N – A fluid property module for the TOUGH2 code for studies of CO2 storage in saline aquifers. *Energy Conversion and Managemen*t, **2007**, *48 (6)*: 1761–1767.

Réveillère, A.; Rohmer, J.; Manceau, J-C. Hydraulic barrier design and applicability for managing the risk of CO2 leakage from deep saline aquifers. *International Journal of Greenhouse Gas Control* **2012**, *9*: 62-71. Accessed 5 September 2012 @ URL: <http://www.sciencedirect.com/science/article/pii/S1750583612000564>.

Sharqawy, M. H.; Lienhard, J. H.; Zubair, S. M. Thermophysical properties of seawater: a review of existing correlations and data. *Desalination and Water Treatment* **2010**, *16 (1-3)*: 354–380. Accessed 23 July 2012 @ URL: <http://web.mit.edu/lienhard/www/Thermophysical_properties_of_seawater-DWT-16-354-2010.pdf>

Span, R.; Wagner, W. A new equation of state for carbon dioxide covering the fluid region from the triple-point temperature to 1100 K at pressures up to 800 MPa: *Journal of Physical and Chemical Reference Data* **1996**, *25 (6)*: 1509–1597.

Spycher, N.; Pruess, K. CO2–H2O mixtures in the geological sequestration of CO2. II. Partitioning in chloride brines at 12–100oC and up to 600 bar. *Geochimica et Cosmochimica Acta* **2005**, *69 (13)*: 3309-3320. {Also: Berkeley, CA: Lawrence Berkeley National Laboratory, 2004. Accessed on 27 July 2012 @ URL: <http://escholarship.org/uc/item/2z23v4zc#page-1>.

Spycher, N.; Pruess, K.; Ennis-King, J. CO2–H2O mixtures in the geological sequestration of CO2. I. Assessment and calculation of mutual solubilities from 12 to 100oC and up to 600 bar. *Geochimica et Cosmochimica Acta* **2003**, *67 (16)*: 3015–3031.

Standing, M. B.; Katz, D. L. Density of natural gases. *Transactions AIME* 1942; 146, p. 140.

Sulston, W. J. The temperature variation of the viscosity of aqueous solutions of strong electrolytes. *Proceedings of the Physical Society* **1935**, *47 (4)*: 657-666.

Sun, H.; Feistel, R.; Koch, M.; Markoe, A. New equations for density, entropy, heat capacity, and potential temperature of a saline thermal fluid. *Deep-Sea Research Part I, Oceanographic Research Papers,* 2008; 55 (10): 1304– 1310. Accessed on 27 August 2012 @ URL: <http://www.uni-kassel.de/fb14/geohydraulik/koch/paper/2008/State_Thermal_Fluid.pdf>

Takenouchi, S.; Kennedy, G. C. The solubility of carbon dioxide in NaCl solutions at high Temperatures and pressures. *American Journal of Science* **1965**, *263 (5)*: 445– 454.

Viswanath, D. S.; Ghosh, T. K.; Prasad, D. H. L.; Dutt, N. V. K.; Rani, K. Y. *Viscosity of liquids: Theory, Estimation, Experiment, and Data*. Dordrecht, Netherlands: Springer, 2007.

Wagner, W. P.; Pruss, A. The IAPWS formulation 1995 for the thermodynamic properties of ordinary water substance for general and scientific use. *Journal of Physical and Chemical Reference Data* **2002**, 31 (2): 387-535.

Wischnewski, B. *CalcSteam.* (Software, Apple App). Berlin, Germany: Peace Software, 2012. Accessed 26 July 2012 @ URL: <http://www.peacesoftware.de/apps/steam_e.html>.