{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":14,"n_cols":29,"rows_kept":14,"cut":false,"hidden":false,"merged":[]}
["Citizen Green #1","Solid phase chemistry","Lower Sidewalls + Reservoir Sand Samples","WC = Whole Core"]
["Quant XRD + Standard Petrophysics","Compiled by J. Ajo-Franklin & M. Voltolini","2013-04-27"]
[{"$nulls":4},"Flow Properties",null,"Quant XRD Weight %"]
[null,"Wireline Depth (ft)","TVD (ft)","Formation","Porosity (Helium %)","Permeability (gas, mD)","Quartz (%)","Quartz (error)","K-Feldspar (%)","K-Feldspar (error)","Albite (%)","Albite (error)","Labradorite (%)","Labrodorite (error)","Andesine (%)","Andesine (error)","Kaolinite (%)","Kaolinite (error)","Chlorite (%)","Chlorite (error)","Pyrite (%)","Pyrite (error)","Amphibole (Fe-Horneblende) %","Amphibole (error)","Sepiloite (%)","Sepiolite (error)","Detrital Mica (%)","Detrital Mica (error)","Montmorillonite"]
[8,7136,6492.3,"Top Starkey Sand",31.4,432.6,42.825294,1.093,8.6653199999999995,0.85653599999999996,0,0,0,0,39.57602,1.4782999999999999,1.3892618000000001,0.35297699999999999,4.6722793999999999,0.45915499999999998,0.45347999999999999,0.139263,"(trace?)",0,0,0,2.4183439999999998,0.58034664000000002,0]
[9,7104,6460.9,"Top Starkey Sand",27.6,114.3,39.880279999999999,0.42972300000000002,6.5165610000000003,0.17615,0,0,0,0,27.354672999999998,0.60929,5.6634640000000003,0.44129000000000002,8.5061319999999991,0.51124999999999998,1.2477217,0.147536,0,0,1.3393781,0.19645662999999999,9.4917929999999995,0.59886399999999995,0]
[15,6936,6296.8,"H&T Shale (sand stringer)",34.200000000000003,299.89999999999998,44.121062999999999,0.40501900000000002,16.600072999999998,0.337001,0,0,0,0,30.431965000000002,0.43622699999999998,4.2134457000000003,0.34288000000000002,4.4872065000000001,0.40515000000000001,0,0,0,0,0,0,0.14624651,0.4589355,0]
[21,6598,5970.1,"Mokelumne River Fm.",31.3,135.5,33.924835000000002,1.0885199999999999,21.998176999999998,1.10104,0,0,0,0,34.475430000000003,1.52196,3.6258416000000002,0.44828400000000002,5.4110084000000001,0.62217,0.21306600000000001,0.15257000000000001,0.23096700000000001,0.30677500000000002,0,0,0.12067264,0.57176815999999997,0]
[22,null,null,"Mokelumne River Fm",null,null,34.200000000000003,null,24.1,null,0,null,0,null,31,null,2.9,null,2,null,0.5,null,1.1000000000000001,null,null,null,4.2]
[23,6466,5843.1,"Mokelumne River Fm.",31.3,71.900000000000006,36.325405000000003,1.79403,12.587688999999999,2.6741999999999999,0.22734215999999999,0.48343000000000003,36.583590000000001,6.7053700000000003,0,0,2.6778168999999998,0.34699999999999998,5.3593655,0.44974399999999998,0.69619757000000004,0.16844000000000001,0.56952630000000004,0.21495785000000001,0,0,4.9730654000000003,0.66014430000000002,0]
[24,6400,5780.1,"Mokelumne River Fm.",33,367.1,40.309690000000003,0.5161,17.08427,0.61682000000000003,0,0,29.232862000000001,0.64956199999999997,3.6258943000000001,0.82246600000000003,5.2308919999999999,0.48113400000000001,3.9868907999999998,0.57289000000000001,0,0,0.17200066,0.52136194999999996,0,0,0.35749905999999998,0.65387832999999995,0]
[]
["WC (shale baffle)",5249,4725.2,"Mokelumne River Fm.","NA","NA",17,"-",32.700000000000003,"-",6.5,"-",0,"-",0,"-",34.9,"-",0,0,0,"-",0,"-",0,"-",8.4,"-","trace"]
["WC (top reservoir sand)",5247,4723.5,"Mokelumne River Fm.","NA","NA",27.8,"-",16.2,"-",34,"-",0,"-",0,"-",3.6,"-",17,0,0,"-",0,"-",0,"-",0,"-",1.1000000000000001]